Algorithm Grid (Inverse distance to a power) starting...
GDAL command:
gdal_grid -l "Lumps 2013" -zfield Cat_Num -a invdist:power=2:smothing=0:radius1=0:radius2=0:angle=0:max_points=0:min_points=0:nodata=0 -ot Float32 "/Users/donaldatkinson/Desktop/QGIS Errors/Lumps 2013.shp" /var/folders/t3/3vvmbd315dv8jgh0n8g4yy0h0000gn/T/processing/f0dbbc541bc44cbe9934108137579be6/OUTPUT.tif 
GDAL command output:
Grid data type is "Float32" 
Grid size = (256 256). 
Corner coordinates = (-60.758630 57.695719)-(-46.899704 42.762614). 
Grid cell size = (0.053926 0.058105). 
Source point count = 1125. 
Algorithm name: "invdist". 
Options are "power=2.000000:smoothing=0.000000:radius1=0.000000:radius2=0.000000:angle=0.000000:max_points=0:min_points=0:nodata=0.000000" 
 
0...10...20...30...40...50...60...70...80...90...100 - done. 
Converting outputs
Loading resulting layers
Algorithm Grid (Inverse distance to a power) finished